|  | 9.7 |
Range of Equipment for Testing Structured Cabling Projects
| 9.7.12 |
Using a cable tester to locate sources of outside interference
To use a cable tester to take a noise reading on a cable, you should disconnect all cables from the computer equipment. High reading levels usually indicate a problem. A simple way to locate the precise source is to unplug each electrical device until the source of the noise is found. Be aware, however, that this does not always work.
| Web Links
| Cabling Glossary
| Network Test Equipment