| Lab 10.4.1 IP Addressing Overview Estimated time: 30 min. Objectives: This Lab will focus on your ability to accomplish the following tasks: Name the five different classes of IP addresses Describe the characteristics and use of the different IP address classes Identify the Class of an IP address based on the network number Determine which part (octets) of an IP address is the network ID and which part is the host ID Identify valid and invalid IP host addresses based on the rules of IP addressing Define the range of addresses and default subnet mask for each class Background: This lab will help you develop an understanding of IP addresses and how TCP/IP networks operate. IP addresses are used to uniquely identify individual TCP/IP networks and hosts (computers and printers) on those network in order for devices to communicate. Workstations and servers on a TCP/IP network are called "HOSTS" and each will have a unique IP address which is referred to as its "HOST" address. TCP/IP is the most widely used protocol in the world. The Internet or World Wide Web uses only IP addressing. In order for a host to access the Internet, it must have an IP address. In its basic form, the IP address has two parts; a Network Address and a Host Address. The network portion of the IP address is assigned to a company or organization by the Internet Network Information Center (InterNIC). Routers use the IP address to move data packets between networks. IP Addresses are 32 bits long (with current version IPv4) and are divided into 4 octets of 8 bits each. They operate at the network layer, Layer 3 of the OSI model, (the Internetwork Layer of the TCP/IP model) and are assigned statically (manually) by a network administrator or dynamically (automatically) by a Dynamic Host Configuration Protocol (DHCP) Server. The IP address of a workstation (host) is a "logical address" meaning it can be changed. The MAC address of the workstation is a 48-bit "physical address" which is burned into the NIC and cannot change unless the NIC is replaced. The combination of the logical IP address and the physical MAC address help route packets to their proper destination. There are 5 different classes of IP addresses and depending on the class, the network and host part of the address will use a different number of bits. In this lab you will work with the different classes of IP addresses and become familiar with the characteristics of each. The understanding of IP addresses is critical to your understanding of TCP/IP and Internetworks in general. Tools / Preparation: This is primarily a written lab exercise but you may want to use Control Panel / Network to review some real network IP addresses. The following resources will be required: PC workstation with Windows operating system (Win 95, 98, NT or 2000) installed on PC and access to the Windows Calculator. Notes: Step 1 – Review IP Address classes and Their Characteristics. Explanation: There are 5 classes of IP addresses (A thru E). Only the first 3 classes are used commercially. We will discuss a class A network address in the table to get started. The first column is the class of IP address. The second column is the first octet which must fall within the range shown for a given class of address. The class A address must start with a number between 1 and 126. The first bit of a class "A" address is always a zero meaning the High Order Bit (HOB) or the 128 bit cannot be used. 127 is reserved for loop back testing. The first octet alone defines the network ID for a class A network address. The default subnet mask uses all binary ones (decimal 255) to mask the first 8 bits of the class A address. The default subnet mask helps routers and hosts determine if the destination host is on this network or another one. Since there are only 126 class A networks, the remaining 24 bits (3 octets) can be used for hosts. Each class A network can have 2^24 power (2 to the 24th power) or over 16 million hosts. It is common to subdivide the network into smaller groupings called subnets using a custom subnet mask which will be discussed in the next lab. The network or host or host portion of the address can not be all ones or all zeros. As an example, the class A address of 118.0.0.5 is a valid IP address since the network portion (first eight bits equal to 118) is not all zeros and the host portion (the last 24 bits) is not all zeros or all ones. If the host portion were all zeros it would be the network address itself. If the host portion were all 1's it would be a broadcast for the network address. The value of any octet can never be greater than decimal 255 or binary 11111111.
Cls | 1st Octet Decimal Range | 1st Octet High Order Bits | Network / Host ID (N=Network, H=Host) | Default Subnet Mask | Number of Networks | Hosts per Network (usable addresses)
A | 1 – 126* | 0 | N.H.H.H | 255.0.0.0 | 126 (27 – 2) | 16,777,214 (2 24 – 2)
B | 128 – 191 | 1 0 | N.N.H.H | 255.255.0.0 | 16,382 (214 - 2) | 65,534 (2 16 – 2)
C | 192 – 223 | 1 1 0 | N.N.N.H | 255.255.255.0 | 2,097,150 (221 – 2) | 254 (2 8 – 2)
D | 224 – 239 | 1 1 1 0 | Reserved for Multicasting
E | 240 – 254 | 1 1 1 1 0 | Experimental, used for research
> * Class A address 127 cannot be used and is reserved for loopback and diagnostic functions Step 2 - Basic IP Addressing. Task: Use the IP address chart and your knowledge of IP address classes to answer the following questions. What is the decimal and binary range of the first octet of all possible class "B" IP addresses? Decimal: From: ________ To: ________ Binary: From: ________ To: ________ Which octet(s) represent the network portion of a class C IP address? ______________ Which octet(s) represent the host portion of a class "A" IP address? ________________ Step 3 – Determine the host and network portion of the IP address. Task: With the following IP host addresses, indicate the Class of each address, the Network Address or ID, the Host portion, the Broadcast Address for this network and the default Subnet Mask. Explanation: The host portion will be all zeros for the network ID. Enter just the octets that make up the host. The host portion will be all ones for a broadcast. The network portion of the address will be all ones for the subnet mask. Fill in the following table:
> Host IP Address | Addr.Class | Network Address | Host Address | Network Broadcast Address | Default Subnet Mask
> 216.14.55.137 |  |  |  |  |
> 123.1.1.15 |  |  |  |  |
> 150.127.221.244 |  |  |  |  |
> 194.125.35.199 |  |  |  |  |
> 175.12.239.244 |  |  |  |  |
Given an IP address of 142.226.0.15 What is the binary equivalent of the second octet? ___________________ What is the Class of the address? _________________________________ What is the network address of this IP address? ____________________ Is this a valid IP host address (Y/N) ? _____________________________ Why or why not? _______________________________________________________ _____________________________________________________________________ _____________________________________________________________________ _____________________________________________________________________ Which is the maximum number of hosts you can have with a class C network address? ______ How many class B networks are there? _____________ How many hosts can each class B network have ? ______________ How many octets are there in an IP address? ________ How many bits per octet? ________ Step 4 – Determine which IP host addresses are valid for commercial networks. Task: For the following IP host addresses determine which are valid for commercial networks. Why or why not?. Explanation: Valid means it could be assigned to a workstation, server, printer, router interface etc. Fill in the following table.
IP Address | Valid Address? (Yes/No) | Why or why not?
150.100.255.255 |  |
175.100.255.18 |  |
195.234.253.0 |  |
100.0.0.23 |  |
188.258.221.176 |  |
127.34.25.189 |  |
224.156.217.73 |  |