|  | 8.4 | Planning Structured Cabling: Selection Practice
| 8.4.9 | Closet H
Potential wiring closet H is a little larger than room G. Its dimensions are approximately 2.4 m wide x .9 m deep. Although its door is .9 m wide, entry into room G is through a small narrow hallway. When the door opens, it swings into the room. Water pipes run through the dropped ceiling space of the room. High voltage electrical conduits also pass through the room. Lighting is provided by an overhead incandescent light; however, the switch that turns the light on and off is located outside the doorway into the room. The floor is carpeted. There is no heating or cooling vent into the room, nor does any heating and cooling ductwork pass through the dropped ceiling space of this room. The nearest thermostat is located in the main corridor, around the corner. There is just one electrical outlet in room G. It is located along the wall that separates room G from the men's room.