Chapter 5: Layer 1 - Media, Connections and Collisions Labs:
5.3.1 | In this lab, your instructor will give you functional, intermittent, and bad cables (Ethernet 10Base-T RJ-45 568-B) to test for continuity, using the Fluke 620 cable tester (or its equivalent).
5.3.2 | In this lab, you will use the following steps to make and test a straight-through patch cable. As specified in the 568 standards, your cable may have a maximum length of 3 m.
5.3.3 | In this lab, you will make, and test a rollover or console cable. This cable is used to connect a PC to the router for purposes of accessing the router.
5.3.4 | In this lab, you will make and test a cross-over cable. Cross-over cables are used to connect one device to another.
5.3.5 | In this lab, you will learn the advanced features of the Fluke 620 LAN CableMeter (or its equivalent).
5.3.6 | In this lab, you will perform cable identification experiments using the Fluke 620 LAN CableMeter (or its equivalent).
5.3.7 | In this lab you, will perform length measurements using the Fluke 620 LAN CableMeter (or its equivalent).