|  | 8.4 | Planning Structured Cabling: Selection Practice
| 8.4.2 | Closet A
Location A is a small closet approximately .9 m wide x 2.4 m deep. It has a dropped ceiling with fluorescent lighting. The switch that turns the light on and off is located just inside the closet door. The floor is carpeted and the walls are of concrete block construction. There is only one electrical outlet in the closet. It is located on the back wall. Currently the room is used to store office supplies. Although a heating and cooling duct passes through the dropped ceiling space over the room, there is no vent into the room. The nearest thermostat for this section of the building is located in Room 113. The door swings outward when it opens, and is approximately .9 m wide. However, because all of the staff members must be able to access the storage area, there is no lock on the door.