|  | 9.2 | RJ-45 Jack and Outlet Installation
| 9.2.10 | Flush mounting a jack in a wall
After you have prepared an opening in which to position the jack, you can then place it in the wall. If you are using a box for mounting the jack, hold the cable, and feed it through one of the slots into the box; then, push the box into the wall opening. Use the screws to secure the box to the wall's surface. As you tighten the screws, the box will be pulled tighter to the wall. If you are mounting the jack in a low-voltage mounting bracket, place the bracket against the wall opening - the smooth side facing outward. Push the top and bottom flanges toward the back, so that the bracket grips the wall. Then, push one side up and the other down, to securely mount the bracket.
| Web Links
| Cabling Glossary
| Cable Termination and Installation